
# Before Patient Arrives

Setting up the camera

1. Set up the tripod at a reasonable height to image the patient. Make sure that the bubble on the level is in the center.
2. Set camera up on tripod by attaching it to the base plate using the screw to secure it so it does not move.
3. Turn on laptop
4. Plug one end of the USB into the laptop and the other end into the camera
5. Open the **IR Flash** software on the laptop
   1. You should be able to see a live image showing up
6. Make sure the image is **Gray Scale**
7. **Unselect the AGC box**
8. Adjust the **Min** and **Max** values based on the histogram to have the best contrast
   1. Generally, min around 23 and max around 38
9. Set **Averaging** to **30**

Setting up Image Series Capture

1. Select Video 🡪 Capture Image Settings
2. Set Capture Type to “Capture for fixed time”
3. Set Time to 0 hours 15 minutes 0 seconds
4. Change Capture Rate to 2 Per Minute
5. Select OK

Chair Setup

# After Patient Arrives

Adjust Chair Setup

Image Ruler

* Save ruler image

Image Right and Left (Initial)

* Save right and left then delete them

Image Front

* Use save all

Image Right and Left (Final)